CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.2/conf/instr/spect/uxnmr.info
Date         : Fri Mar  4 12:41:49 2022
Release      : TOPSPIN Version 3.2-pl5
Installed in : /opt/topspin3.2
Host         : CZC34002ZQ
OS           : CentOS release 5.11 (Final)
CPU          : Intel(R) Xeon(R) CPU E5-1620 0 @ 3.60GHz (8 cores at 1200 MHz with Hyperthreading)
User         : pedro
Description  : AVHD600XWB
Location     : TU Darmstadt
System       : Avance III NMR spectrometer
1H-frequency : 600.13 MHz
Order Number : 10121075
Configured in: /opt/topspin3.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.251
- Tctrl : 1
- Fctrls: 3
- Gctrl : none
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/03648 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 130419
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x43   0x5    CD  R  0.2 REC-1  AQS RXAD/2 600 Z130588/693 ECL 00.02
     3   0x34 0xd6   0x1        X  3.1 REF-1  REF/3-600 Reference Board for AQS/3 Receiver
     4   0x24 0x32     0        S  2.2 SGU-1  AQS SGU/3 600 (2CH) Z117129/01117 ECL 02.02 FPGA-Vs=20131031
     5   0x26 0x32     0        S  2.2 SGU-2  AQS SGU/3 600 (2CH) Z117129/01216 ECL 02.02 FPGA-Vs=20131031
    10   0x3c 0xc5     0        Y  1.0 ROUT-1 AQS Router 1/4
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 AQS Router 1/4


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0608 W1345093/0608 ECL 12:
- TCP/IP address = 149.236.99.254
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0608 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2322 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7258 ECL 50
BLA_W1345092_0665 W1345092/0665 ECL 11:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ INR: W1345092/0665 ECL 11
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2532 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7699 ECL 50
BLA_W1345087_0225 W1345087/0225 ECL 30:
- TCP/IP address = 149.236.99.246
- Firmware VS    = 20120627
- Amplifier      = BLAH300 E 200-600MHZ INR: W1345087/0225 ECL 30
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2487 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7418 ECL 50

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20130320
- SCB channels = 40
- Shim System = BOSS-WB
- 2HTX Amplifier: not available
- Lock: not available
- VTU_SPB = BSMS/2 SPB-E SENSOR & PNEUMATIC BD: Z115192/00312 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01886 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

MAS2 control unit: connected to 149.236.99.251:/dev/tty04
- Boot Software        : 20100908
- Application Software : 20130715
- Insert Time          : 10 s
- Eject Time           : 10 s
- Spin Lock Tolerance  : 5 Hz

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.0%/0.1deg, reflection meter)
                 PN=Z103205, SN=00268 from 20131016
    Module  2 : XBB19F 2HP
                 PN=Z105186, SN=00008 from 20131001
    Module  3 : XBB19F 2HP
                 PN=Z105186, SN=00009 from 20131001


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0608 at TCP/IP 149.236.99.254)
SGU1 AUX  output -> open
SGU2 NORM output -> input 1 of transmitter 3 (BLAH300 E 200-600MHZ INR W1345087/0225 at TCP/IP 149.236.99.246)
SGU2 AUX  output -> open
SGU3 NORM output -> input 1 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0665 at TCP/IP 149.236.99.252)
SGU3 AUX  output -> input of AQS Router 1/4
AQS Router 1/4 output 1 -> input 2 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0608 at TCP/IP 149.236.99.254)
AQS Router 1/4 output 2 -> input 2 of transmitter 3 (BLAH300 E 200-600MHZ INR W1345087/0225 at TCP/IP 149.236.99.246)
AQS Router 1/4 output 3 -> input 2 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0665 at TCP/IP 149.236.99.252)
AQS Router 1/4 output 4 -> open

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0608 at TCP/IP 149.236.99.254) amplifier X-500W uses blanking 1
transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0665 at TCP/IP 149.236.99.252) amplifier X-300W uses blanking 3
transmitter 3 (BLAH300 E 200-600MHZ INR W1345087/0225 at TCP/IP 149.236.99.246) amplifier 1H-300W uses blanking 2
transmitter 3 (BLAH300 E 200-600MHZ INR W1345087/0225 at TCP/IP 149.236.99.246) amplifier 1H-50W uses blanking 2

