CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin/conf/instr/spect/uxnmr.info
Date         : Fri Dec 10 15:10:16 2021
Release      : TopSpin 3.6.2
Installed in : /opt/topspin
Host         : indium.aci.uni-heidelberg.de
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Core(TM) i5-4590 CPU @ 3.30GHz (4 cores at 1849 MHz)
User         : auto (auto)
System       : Avance III 600 NMR spectrometer
1H-frequency : 600.18 MHz
Description  : Avance III 600
Location     : ACI, Uni Heidelberg
Bruker Order : HH005705
Configured in: indium.aci.uni-heidelberg.de:/opt/topspin/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 3
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/00285 ECL 02.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x2    AW  R  1.1 REC-1  AQS RXAD600 Z102117/101 ECL 1.1
     3   0x34 0xc0   0x1        X  0.4 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x29   0x8    AE  S  0.0 SGU-1  AQS SGU/2 1000 Z103082/00047 ECL 00.00 FPGA-Vs=AF
     5   0x25 0x29   0x8    AE  S  0.0 SGU-2  AQS SGU/2 1000 Z103082/00048 ECL 00.00 FPGA-Vs=AF
     6   0x26 0x29   0x8    AE  S  0.0 SGU-3  AQS SGU/2 1000 Z103082/00078 ECL 00.00 FPGA-Vs=AF
    21   0x21 0xcf     0        P  0.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xc6     0        B  1.1 AQS/2  AQS/2 chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345092_0003 W1345092/0003 ECL 0:
- TCP/IP address = 149.236.99.92
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ: W1345092/0003 ECL 0
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0018 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V V-USB: W1522040/0032 ECL 0
BLA_W1345096_0003 W1345096/0003 ECL 0:
- TCP/IP address = 149.236.99.91
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ: W1345096/0003 ECL 0
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0007 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V V-USB: W1522040/0043 ECL 0

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20180919
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS2-SB
- 2HTX Amplifier: not available
- Lock: installed

Bruker Automatic Changer: device connected to 149.236.99.90:/dev/tty05
- Capacity: 60 holders
- Firmware: 20040805
- use BACS air  = yes
- BACS sx delay = 1 s
- Sample Rail fast changer mode = no

Eurotherm VTU: device connected to 149.236.99.90:/dev/tty04

Cryo Cooling Control Unit: CU5 - COOLING UNIT/5 Z159072/258
- TCP/IP address   = 149.236.99.94

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                PN=Z003462, SN=00424 from 20051123
    Module  2 : XBB19F 2HS
                PN=Z003506, SN=00444 from 20051103
    Module  3 : 2H
                PN=Z003473, SN=00426 from 20051124



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0003 at TCP/IP 149.236.99.91)
SGU1 AUX  output -> input 1 of transmitter 1 (BLAX300 E 6-365MHZ W1345092/0003 at TCP/IP 149.236.99.92)
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0003 at TCP/IP 149.236.99.91)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 2 of transmitter 1 (BLAX300 E 6-365MHZ W1345092/0003 at TCP/IP 149.236.99.92)
SGU3 AUX  output -> input 4 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0003 at TCP/IP 149.236.99.91)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX300 E 6-365MHZ W1345092/0003 at TCP/IP 149.236.99.92:
- amplifier X-300W uses blanking 3

transmitter 2 = BLAXH2H300/100/150 E 200-600MHZ W1345096/0003 at TCP/IP 149.236.99.91:
- amplifier 1H-100W uses blanking 2
- amplifier X-300W uses blanking 1
- amplifier 2H-150W needs no blanking


