Caption:
Steady-state velocity magnitude and streamlines at $\Omega=1000$\,rpm. The kinematic viscosity for the calculations was set as $\nu_{\text{D}_\text{w}}=8.1614\cdot10^{-6}\,\mathrm{m}^2/\mathrm{s}$, estimated from the values of Gontrani et al. [150] for $\eta_{\text{D}_\text{w}}$ at 80\,$^\circ$C and $\rho_{\text{D}_\text{w}}$ from Florindo et al. [128] at 75\,$^\circ$C, which was the only value found for density at elevated temperatures. The indicated wavelength $\lambda_1\approx5.6\,$mm is greater than the wavelengths of the other vortex pairs with $\overline{\lambda}=5.4\,$mm.

Notes:
[128] Florindo, C., Oliveira, F. S., Rebelo, L. P. N., Fernandes, A. M., & Marrucho,
I. M. (2014). Insights into the synthesis and properties of deep eutectic solvents
based on cholinium chloride and carboxylic acids. ACS Sustainable Chemistry
& Engineering, 2(10):2416–2425. DOI: https://doi.org/10.1021/sc500439w.

[150] Gontrani, L., Bonomo, M., Plechkova, N. V., Dini, D., & Caminiti, R. (2018).
X-ray structure and ionic conductivity studies of anhydrous and hydrated choline
chloride and oxalic acid deep eutectic solvents. Phys. Chem. Chem. Phys.,
20:30120–30124. DOI: https://doi.org/10.1039/C8CP06728G.

Case data variables:
Position in x-direction in m: Points:0
Position in y-direction in m: Points:1
Position in z-direction in m: Points:2

Velocity U in x-direction in m/s: U:0
Velocity U in y-direction in m/s: U:1
Velocity U in z-direction in m/s: U:2

Pressure p in Pa: p

