# General

This folder contains the individual acoustic emissions without further processing and without division into training, validation, and test data.

# Naming Convention

The naming convention for the plates is:
{MountingType}\_P{PlateNumber}\_{PlateSide}\_D{RunNumber}\_{PointNumber}  
The plate number can be found on its label.
Plate side A is the side with the plate number label.
The point number follows this scheme:

```
            Side A
01  07  13  19  25  31  37  43
02  08  14  20  26  32  38  44
03  09  15  21  27  33  39  45
04  10  16  22  28  34  40  46
05  11  17  23  29  35  41  47
06  12  18  24  30  36  42  48
```

Piercing through point XX on side A will always lead to the exact same point XX on side B.

# Labels

Plates 1-4 are completely intact.  
Plates 5 and 6 have defects at the following sampling points: 9, 10, 15, 16, 32, 35, 38, 41.  
Plate 7 has defective areas at: 25-30.  
The additional files for Plate 7 are all from defective areas.  
Plate 8 has defective areas at: 19-30.  
Plates 1-4 that are labeled with "Schlagschaden" (impact damage) are all defective.